(module WLP4_0P82X0P82_MEM (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS)
    (effects (font (size 1 1) (thickness .15)))
  )
  (fp_text value WLP4_0P82X0P82_MEM (at 0 0) (layer F.SilkS)
    (effects (font (size 1 1) (thickness .15)))
  )
  (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User)
    (effects (font (size .127 .127) (thickness .002)))
  )
  (fp_text user "*" (at 0 0) (layer F.SilkS)
    (effects (font (size 1 1) (thickness .15)))
  )
  (fp_text user "*" (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness .15)))
  )
  (fp_text user "A" (at -1.0541 -.2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness .15)))
  )
  (fp_text user "A" (at -1.0541 -.2) (layer F.Fab)
    (effects (font (size 1 1) (thickness .15)))
  )
  (fp_text user "A" (at -1.0541 -.2) (layer B.SilkS)
    (effects (font (size 1 1) (thickness .15)))
  )
  (fp_text user "B" (at -1.0541 .2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness .15)))
  )
  (fp_text user "B" (at -1.0541 .2) (layer F.Fab)
    (effects (font (size 1 1) (thickness .15)))
  )
  (fp_text user "B" (at -1.0541 .2) (layer B.SilkS)
    (effects (font (size 1 1) (thickness .15)))
  )
  (fp_text user "1" (at -.2 -1.0541 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness .15)))
  )
  (fp_text user "1" (at -.2 -1.0541 90) (layer F.Fab)
    (effects (font (size 1 1) (thickness .15)))
  )
  (fp_text user "1" (at -.2 -1.0541 90) (layer B.SilkS)
    (effects (font (size 1 1) (thickness .15)))
  )
  (fp_text user "2" (at .2 -1.0541 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness .15)))
  )
  (fp_text user "2" (at .2 -1.0541 90) (layer F.Fab)
    (effects (font (size 1 1) (thickness .15)))
  )
  (fp_text user "2" (at .2 -1.0541 90) (layer B.SilkS)
    (effects (font (size 1 1) (thickness .15)))
  )
  (fp_text user "0.2in/5.08mm" (at -2.8321 0) (layer Cmts.User)
    (effects (font (size 1 1) (thickness .15)))
  )
  (fp_text user "0.15in/3.81mm" (at 0 2.8321) (layer Cmts.User)
    (effects (font (size 1 1) (thickness .15)))
  )
  (fp_text user "0.016in/0.4mm" (at 2.8321 0) (layer Cmts.User)
    (effects (font (size 1 1) (thickness .15)))
  )
  (fp_text user "0.008in/0.203mm" (at 2.8321 .2) (layer Cmts.User)
    (effects (font (size 1 1) (thickness .15)))
  )
  (fp_line (start -.6731 .6731) (end -.6731 -.6731) (layer F.CrtYd) (width .05))
  (fp_line (start -.6731 -.6731) (end .6731 -.6731) (layer F.CrtYd) (width .05))
  (fp_line (start .6731 -.6731) (end .6731 .6731) (layer F.CrtYd) (width .05))
  (fp_line (start .6731 .6731) (end -.6731 .6731) (layer F.CrtYd) (width .05))
  (fp_line (start .2 -.2) (end 2.7051 -.2) (layer Cmts.User) (width 0))
  (fp_line (start .2 .2) (end 2.7051 .2) (layer Cmts.User) (width 0))
  (fp_line (start 2.3241 -.2) (end 2.3241 -1.47) (layer Cmts.User) (width 0))
  (fp_line (start 2.3241 .2) (end 2.3241 1.47) (layer Cmts.User) (width 0))
  (fp_line (start 2.3241 -.2) (end 2.1971 -.454) (layer Cmts.User) (width 0))
  (fp_line (start 2.3241 -.2) (end 2.4511 -.454) (layer Cmts.User) (width 0))
  (fp_line (start 2.1971 -.454) (end 2.4511 -.454) (layer Cmts.User) (width 0))
  (fp_line (start 2.3241 .2) (end 2.1971 .454) (layer Cmts.User) (width 0))
  (fp_line (start 2.3241 .2) (end 2.4511 .454) (layer Cmts.User) (width 0))
  (fp_line (start 2.1971 .454) (end 2.4511 .454) (layer Cmts.User) (width 0))
  (fp_line (start -.4191 0) (end -.4191 -2.7051) (layer Cmts.User) (width 0))
  (fp_line (start .4191 0) (end .4191 -2.7051) (layer Cmts.User) (width 0))
  (fp_line (start -.4191 -2.3241) (end -1.6891 -2.3241) (layer Cmts.User) (width 0))
  (fp_line (start .4191 -2.3241) (end 1.6891 -2.3241) (layer Cmts.User) (width 0))
  (fp_line (start -.4191 -2.3241) (end -.6731 -2.4511) (layer Cmts.User) (width 0))
  (fp_line (start -.4191 -2.3241) (end -.6731 -2.1971) (layer Cmts.User) (width 0))
  (fp_line (start -.6731 -2.4511) (end -.6731 -2.1971) (layer Cmts.User) (width 0))
  (fp_line (start .4191 -2.3241) (end .6731 -2.4511) (layer Cmts.User) (width 0))
  (fp_line (start .4191 -2.3241) (end .6731 -2.1971) (layer Cmts.User) (width 0))
  (fp_line (start .6731 -2.4511) (end .6731 -2.1971) (layer Cmts.User) (width 0))
  (fp_line (start 0 -.4191) (end 4.6101 -.4191) (layer Cmts.User) (width 0))
  (fp_line (start 0 .4191) (end 4.6101 .4191) (layer Cmts.User) (width 0))
  (fp_line (start 4.2291 -.4191) (end 4.2291 -1.6891) (layer Cmts.User) (width 0))
  (fp_line (start 4.2291 .4191) (end 4.2291 1.6891) (layer Cmts.User) (width 0))
  (fp_line (start 4.2291 -.4191) (end 4.1021 -.6731) (layer Cmts.User) (width 0))
  (fp_line (start 4.2291 -.4191) (end 4.3561 -.6731) (layer Cmts.User) (width 0))
  (fp_line (start 4.1021 -.6731) (end 4.3561 -.6731) (layer Cmts.User) (width 0))
  (fp_line (start 4.2291 .4191) (end 4.1021 .6731) (layer Cmts.User) (width 0))
  (fp_line (start 4.2291 .4191) (end 4.3561 .6731) (layer Cmts.User) (width 0))
  (fp_line (start 4.1021 .6731) (end 4.3561 .6731) (layer Cmts.User) (width 0))
  (fp_line (start -.2191 -.4191) (end -.4191 -.2191) (layer F.Fab) (width .1))
  (fp_line (start -.4191 .4191) (end .4191 .4191) (layer F.Fab) (width .1))
  (fp_line (start .4191 .4191) (end .4191 -.4191) (layer F.Fab) (width .1))
  (fp_line (start .4191 -.4191) (end -.4191 -.4191) (layer F.Fab) (width .1))
  (fp_line (start -.4191 -.4191) (end -.4191 .4191) (layer F.Fab) (width .1))
  (fp_line (start -.6731 .6731) (end -.6731 -.6731) (layer F.CrtYd) (width .05))
  (fp_line (start -.6731 -.6731) (end .6731 -.6731) (layer F.CrtYd) (width .05))
  (fp_line (start .6731 -.6731) (end .6731 .6731) (layer F.CrtYd) (width .05))
  (fp_line (start .6731 .6731) (end -.6731 .6731) (layer F.CrtYd) (width .05))
  (pad A1 smd circle (at -.2 -.2) (size .2032 .2032) (layers F.Cu F.Paste F.Mask))
  (pad A2 smd circle (at .2 -.2) (size .2032 .2032) (layers F.Cu F.Paste F.Mask))
  (pad B1 smd circle (at -.2 .2) (size .2032 .2032) (layers F.Cu F.Paste F.Mask))
  (pad B2 smd circle (at .2 .2) (size .2032 .2032) (layers F.Cu F.Paste F.Mask))
)
